##---------------------------------------------------
## 2005 Nissan Skyline GT-R R34 NISMO Z-Tune
## Replacement for Fiat Punto
## Attributes.bin patch script
##---------------------------------------------------

memfile GLOBAL\GlobalMemoryFile.bin
vpak GLOBAL\ATTRIBUTES.BIN db


##---------------------------------------------------
## Node: pvehicle/default/cars/racers/punto
##---------------------------------------------------

## TurboSND[0]
patch	int32	bin:0x3071c	0x9e45f0b2

## TurboSND[1]
patch	int32	bin:0x3072c	0x9e45f0b2

## TurboSND[2]
patch	int32	bin:0x3073c	0x3f333115

## TurboSND[3]
patch	int32	bin:0x3074c	0x3f333115

## VerbalType; copspeech related; code determines what cops will call your car
## PATCH LENGTH ADDRESS, NOT DATA
patch	int32	bin:0x306f0	0x00008000

## MASS; self-explanatory; mass of car expressed in kilograms
patch	float	bin:0x306e8	1560

## engineaudio[0]
patch	int32	bin:0x30894	0x8d18f209

## engineaudio[1]
patch	int32	bin:0x308a0	0x8d18f209

## engineaudio[2]
patch	int32	bin:0x308ac	0x8d18f209

## TENSOR_SCALE; seems to be overall handling speed scale balancing
## the bigger 2nd value is the slower the car will respond to steering input
## countered by increasing of 1st and 3rd value
patch	float	bin:0x306b0	1
patch	float	bin:0x306b4	2
patch	float	bin:0x306b8	1
patch	float	bin:0x306bc	0

## HandlingRating; used to set min and max handling bars length; doesn't take effect from base or end grip values but its increase is dependent
## on chassis and tires values
## values range from 37-98 for 1st set and 90-100 for 2nd set
patch	float	bin:0x30708	90
patch	float	bin:0x3070c	100

## brakes_upgrades
patch	int32	bin:0x306e4	4

## induction_upgrades
patch	int32	bin:0x306f4	3

## tires_upgrades
patch	int32	bin:0x306ec	3

## engine_upgrades
patch	int32	bin:0x306d8	4

## transmission_upgrades
patch	int32	bin:0x306dc	4

## nos_upgrades
patch	int32	bin:0x306e0	3

## chassis_upgrades
patch	int32	bin:0x306f8	3


##---------------------------------------------------
## Node: ecar/default/racers/punto
##---------------------------------------------------

## BodyDive; maximum vector-based movement of front of car body
## 1st - Degrees/G
## 2nd - Max G
## 3rd - Degrees/sec
patch	float	bin:0x3dd88	2
patch	float	bin:0x3dd8c	10
patch	float	bin:0x3dd90	0.5

## RideHeight; in-race only; visible body height
patch	float	bin:0x3ddcc	0

## TireOffsets
## in format x, y, z, w
## x axis; car front = +; car rear = -
## y axis; left side = +; right = -
## z axis; up = +; down = - note: will move WHEELS [up or down] regarding CAR BODY, during race body will be on normal level
## unlike wheels that might be BELOW ground
## w - wheel diameter scaling; default game values range between 0.31 [elise] and 0.35 [mustanggt]
## NOTE: CAR BODY height will be changed to match wheel size
## all axles have point 0 in center of line between front left and rear right wheel or between front right and rear left

## front left
patch	float	bin:0x3dce0	1.34
patch	float	bin:0x3dce4	0.905
patch	float	bin:0x3dce8	0
patch	float	bin:0x3dcec	0.33

## front right
patch	float	bin:0x3dcf0	1.34
patch	float	bin:0x3dcf4	-0.905
patch	float	bin:0x3dcf8	0
patch	float	bin:0x3dcfc	0.33

## rear right
patch	float	bin:0x3dd00	-1.33
patch	float	bin:0x3dd04	-0.905
patch	float	bin:0x3dd08	0
patch	float	bin:0x3dd0c	0.33

## rear left
patch	float	bin:0x3dd10	-1.33
patch	float	bin:0x3dd14	0.905
patch	float	bin:0x3dd18	0
patch	float	bin:0x3dd1c	0.33

## BodySquat; maximum vector-based movement of rear of car body
## 1st - Degrees/G
## 2nd - Max G
## 3rd - Degrees/sec
patch	float	bin:0x3dd7c	2.5
patch	float	bin:0x3dd80	10
patch	float	bin:0x3dd84	0.5

## CamberRear; angle between the vertical axis of the wheel and the vertical axis of the vehicle
## positive values for bottom of wheel being further out than top, negative for opposite effect
## common value is 0.18
patch	float	bin:0x3ddc8	0.2

## CamberFront; angle between the vertical axis of the wheel and the vertical axis of the vehicle
## positive values for bottom of wheel being further out than top, negative for opposite effect
## common value is 0.22
patch	float	bin:0x3ddc0	0.2

## FECompressions; used to adjust height of car body regarding wheels in frontend menus
## common value range is 2x0.10-2x0.20
patch	float	bin:0x3ddf8	0.14
patch	float	bin:0x3ddfc	0.14

## TireSkidWidth; aka tire width
## common value range is 2x0.225 for front wheels and 2x0.335 for rear wheels
patch	float	bin:0x3ddac	0.275
patch	float	bin:0x3ddb0	0.275
patch	float	bin:0x3ddb4	0.31
patch	float	bin:0x3ddb8	0.31

## WheelSpokeCount; number of spokes in rims
## common value range N/A since it differs per car
patch	int8	bin:0x3ddec	5

## ReflectionOffset; used to fix car's reflection in menus
patch	float	bin:0x3ddc4	0.008

## KitWheelOffsetRear; used to move wheels along axis Y when bodykits are used
## values range from 0 to 128; applies to REAR axle
patch	int8	bin:0x3ddd8	0
patch	int8	bin:0x3ddd9	0
patch	int8	bin:0x3ddda	0
patch	int8	bin:0x3dddb	0
patch	int8	bin:0x3dddc	110
patch	int8	bin:0x3dddd	35

## BodyRoll; maximum vector-based movement of entire car body towards left or right
## simply put - car body leaning sideways
## 1st - Degrees/G
## 2nd - Max G
## 3rd - Degrees/sec
patch	float	bin:0x3dd70	1.7
patch	float	bin:0x3dd74	9
patch	float	bin:0x3dd78	1

## KitWheelOffsetFront; used to move wheels along axis Y when bodykits are used
## values range from 0 to 128; applies to FRONT axle
patch	int8	bin:0x3dde6	0
patch	int8	bin:0x3dde7	0
patch	int8	bin:0x3dde8	0
patch	int8	bin:0x3dde9	0
patch	int8	bin:0x3ddea	80
patch	int8	bin:0x3ddeb	10


##---------------------------------------------------
## Node: brakes/default/punto
##---------------------------------------------------

## BRAKES; overall braking power per axle
## common value range is 300/400-650/700; mass dependent
patch	float	bin:0x244c0	475
patch	float	bin:0x244c4	575

## EBRAKE; handbrake power; should be larger than BRAKES value by at least 10% and larger than overall car horsepower
## common value range is 400-800; mass dependent
patch	float	bin:0x244c8	850

## BRAKE_LOCK; BRAKES field values multiplier and braking force distribution ratio
## common value range is 1.00 for front axle and 3.20-3.60 for rear axle
patch	float	bin:0x244b8	1
patch	float	bin:0x244bc	3.3


##---------------------------------------------------
## Node: brakes/default/punto/punto_top
##---------------------------------------------------

## BRAKES
patch	float	bin:0x24880	585
patch	float	bin:0x24884	675

## EBRAKE
patch	float	bin:0x24888	975

## BRAKE_LOCK
patch	float	bin:0x24878	1
patch	float	bin:0x2487c	3.3


##---------------------------------------------------
## Node: chassis/default/punto
##---------------------------------------------------

## WHEEL_BASE; distance between the centers of the front and rear wheels
## common value range N/A since it differs per car
patch	float	bin:0x8dc0	2.665

## DRAG_COEFFICIENT; air resistance of object travelling in a non-vacuum environment such as air
## common value range is 0.25-0.42
patch	float	bin:0x8ddc	0.3

## SHOCK_VALVING; shock absorber oil flow restriction
## common value range is 2x15-2x24
patch	float	bin:0x8dac	19
patch	float	bin:0x8db0	19

## RIDE_HEIGHT; aka ground clearance
## common value range is 2x6-2x9
patch	float	bin:0x8d84	9
patch	float	bin:0x8d88	9

## SHOCK_STIFFNESS; minimum pressure inside shock absorber in pounds per square inch
## common value range is 2x30-2x80; acceleration and mass-dependent
patch	float	bin:0x8d9c	65
patch	float	bin:0x8da0	67

## SHOCK_BLOWOUT; maximum size by which a dampener can compress in inches; stock same as upgraded
## common value range is 5-8
patch	float	bin:0x8dc4	6

## SHOCK_EXT_STIFFNESS; maximum shock absorber rebound force
## common value range is 2x40-2x80; acceleration-, downforce- and mass-dependent
patch	float	bin:0x8d94	80
patch	float	bin:0x8d98	80

## SWAYBAR_STIFFNESS; self-explanatory; probably expressed in pounds per square inch
## common value range is 2x200-2x450; acceleration and mass dependent
patch	float	bin:0x8db4	400
patch	float	bin:0x8db8	450

## ROLL_CENTER; vertical center of gravity [probably in inches]
## common value range is 8-10
patch	float	bin:0x8dbc	8.5

## TRAVEL; maximum length by which a shock can be extended if car wheels don't have contact with road surface; stock commonly higher than upgraded
## common value range is 2x6-2x8; acceleration and mass dependent
patch	float	bin:0x8d7c	7
patch	float	bin:0x8d80	7

## SPRING_STIFFNESS; overall coilover pressure in pounds square inch
## common value range is 2x400-2x700
patch	float	bin:0x8da4	725
patch	float	bin:0x8da8	675

## AERO_CG; overall distribution of aerodynamic force on the car body; values between 0 and 100; 0 for max in rear, 100 for max in front
## common value range is 47-51
patch	float	bin:0x8dc8	48

## SPRING_PROGRESSION; maximum compression speed/rate for spring to achieve maximum stiffness; stock smaller than upgraded
## higher values will make springs stiffer faster so car won't shove ground on slopes but will also increase bouncing on curbs
## common value range is 2x5-2x8
patch	float	bin:0x8d74	7
patch	float	bin:0x8d78	6.6

## TRACK_WIDTH; axle length; distance between wheels on a single axle; measured in metres
## common value range N/A since it differs per car
patch	float	bin:0x8d8c	1.48
patch	float	bin:0x8d90	1.49

## SHOCK_DIGRESSION; digressive shocks provide smoother ride at higher speeds and absorb body roll also improving cornering; smaller value for smoother ride
## common value range is 2x0.1-2x0.5
patch	float	bin:0x8d6c	0.4
patch	float	bin:0x8d70	0.4

## RENDER_MOTION; dependent on ecar node settings in body roll, dive and squat; used as a multiplier of the mentioned values to calculate car body movement
## common value range is 0.50-1.00
patch	float	bin:0x8dcc	1

## AERO_COEFFICIENT; used to define car aerodynamics factor and overall downforce; value too small will make it slow and too high will push it down to
## ground too hard making it difficult to drive and car will be constantly hitting road due to excessive amount of downforce
## common value range is 0.15-0.30
patch	float	bin:0x8dd4	0.24

## FRONT_AXLE; front axle diameter in inches
## common value range is 1.2-1.5
patch	float	bin:0x8dd0	1.405

## FRONT_WEIGHT_BIAS; overall mass distribution; values from 0 to 100; 0 for max rear bias; 100 for max front bias
## common value range is 51-55
patch	float	bin:0x8dd8	54


##---------------------------------------------------
## Node: chassis/default/punto/punto_top
##---------------------------------------------------

## WHEEL_BASE
patch	float	bin:0x9bcc	2.665

## DRAG_COEFFICIENT
patch	float	bin:0x9be8	0.25

## SHOCK_VALVING
patch	float	bin:0x9bb8	24
patch	float	bin:0x9bbc	24

## RIDE_HEIGHT
patch	float	bin:0x9b90	9
patch	float	bin:0x9b94	9

## SHOCK_STIFFNESS
patch	float	bin:0x9ba8	75
patch	float	bin:0x9bac	69

## SHOCK_BLOWOUT
patch	float	bin:0x9bd0	6

## SHOCK_EXT_STIFFNESS
patch	float	bin:0x9ba0	90
patch	float	bin:0x9ba4	90

## SWAYBAR_STIFFNESS
patch	float	bin:0x9bc0	450
patch	float	bin:0x9bc4	480

## ROLL_CENTER
patch	float	bin:0x9bc8	8.5

## TRAVEL
patch	float	bin:0x9b88	6
patch	float	bin:0x9b8c	6

## SPRING_STIFFNESS
patch	float	bin:0x9bb0	800
patch	float	bin:0x9bb4	775

## AERO_CG
patch	float	bin:0x9bd4	48.5

## SPRING_PROGRESSION
patch	float	bin:0x9b80	8.5
patch	float	bin:0x9b84	8

## TRACK_WIDTH
patch	float	bin:0x9b98	1.48
patch	float	bin:0x9b9c	1.49

## SHOCK_DIGRESSION
patch	float	bin:0x9b78	0.375
patch	float	bin:0x9b7c	0.375

## RENDER_MOTION
patch	float	bin:0x9bd8	1

## AERO_COEFFICIENT
patch	float	bin:0x9be0	0.24

## FRONT_AXLE
patch	float	bin:0x9bdc	1.405

## FRONT_WEIGHT_BIAS
patch	float	bin:0x9be4	54


##---------------------------------------------------
## Node: engine/default/punto
##---------------------------------------------------

## ENGINE_BRAKING; multiplies maximum torque at current gear and uses it to calculate speed loss with no throttle used
## common value range is 0.70-0.90
patch	float	bin:0x12f54	0.7
patch	float	bin:0x12f58	0.8
patch	float	bin:0x12f5c	0.9

## IDLE; minimum operating speed of engine necessary to sustain its work but not enough to move drivetrain components
## common value range is 800-950
patch	float	bin:0x12f6c	800

## TORQUE; self-explanatory; field count suggest game used to support up to 15 torque values; can only use 9 now
## common value range N/A since it differs per car
patch	float	bin:0x12f18	145
patch	float	bin:0x12f1c	167
patch	float	bin:0x12f20	204
patch	float	bin:0x12f24	261
patch	float	bin:0x12f28	315
patch	float	bin:0x12f2c	304
patch	float	bin:0x12f30	279
patch	float	bin:0x12f34	249
patch	float	bin:0x12f38	218

## MAX_RPM; maximum operating speed of engine before its destruction [drag racing only]
## common value range N/A since it differs per car
patch	float	bin:0x12f64	9000

## FLYWHEEL_MASS; the higher the mass, the higher the maximum inertia moment and therefore larger amounts of kinetic energy can be stored
## also the lower the mass, the faster the top speed can be achieved and maintained
## common value range is 9-15
patch	float	bin:0x12f60	11

## RED_LINE; maximum safe operating speed of engine
## common value range N/A since it differs per car
patch	float	bin:0x12f68	8000


##---------------------------------------------------
## Node: engine/default/punto/punto_top
##---------------------------------------------------

## ENGINE_BRAKING
patch	float	bin:0x13fd4	0.7
patch	float	bin:0x13fd8	0.8
patch	float	bin:0x13fdc	0.9

## IDLE
patch	float	bin:0x13fec	800

## TORQUE
patch	float	bin:0x13f98	210
patch	float	bin:0x13f9c	242
patch	float	bin:0x13fa0	295
patch	float	bin:0x13fa4	379
patch	float	bin:0x13fa8	456
patch	float	bin:0x13fac	438
patch	float	bin:0x13fb0	400
patch	float	bin:0x13fb4	358
patch	float	bin:0x13fb8	317

## MAX_RPM
patch	float	bin:0x13fe4	9000

## FLYWHEEL_MASS
patch	float	bin:0x13fe0	11

## RED_LINE
patch	float	bin:0x13fe8	8000


##---------------------------------------------------
## Node: induction/default/punto_base
##---------------------------------------------------

## AIR_PRESSURE*; commonly 0.25
patch	float	bin:0x11ccc	0.25

## HIGH_BOOST
patch	float	bin:0x11ce0	0.125

## LOW_BOOST
patch	float	bin:0x11cc8	0.125

## PSI_ARROW_MOVE_SPEED*; always higher value for stock
patch	float	bin:0x11cd8	2.2

## PSI; maximum pressure of air taken into the turbine
## common value range is 12-15
patch	float	bin:0x11cdc	11

## SPOOL; turbine lag; 0 for 'supercharger'; anything higher will give 'turbo' upgrade
## common value range is 0.00-0.20
patch	float	bin:0x11cd4	0.2

## BOOST_VARIANCE*; pressure drop/rise in chamber
patch	float	bin:0x11cd0	-0.1


##---------------------------------------------------
## Node: induction/default/punto_base/punto_top
##---------------------------------------------------

## AIR_PRESSURE*; commonly 0.25
patch	float	bin:0x120d8	0.25

## HIGH_BOOST
patch	float	bin:0x120ec	0.25

## LOW_BOOST
patch	float	bin:0x120d4	0.25

## PSI_ARROW_MOVE_SPEED*; always higher value for stock
patch	float	bin:0x120e4	2

## PSI; maximum pressure of air taken into the turbine
## common value range is 12-15
patch	float	bin:0x120e8	13

## SPOOL; turbine lag; 0 for 'supercharger'; anything higher will give 'turbo' upgrade
## common value range is 0.00-0.20
patch	float	bin:0x120e0	0.2

## BOOST_VARIANCE*; pressure drop/rise in chamber
patch	float	bin:0x120dc	-0.05


##---------------------------------------------------
## Node: tires/default/punto
##---------------------------------------------------

## SECTION_WIDTH; self-explanatory; measured in milimetres
## common value range N/A since it differs per car
patch	float	bin:0x22690	245
patch	float	bin:0x22694	245

## YAW_CONTROL; equivalent of section-based traction and stability control system; values 1 and 2 for front; values 3 and 4 for rear
## effect similar to dynamic mass bias shifting; highly dependent on WEIGHT_BIAS, AERO_CG, TORQUE_SPLIT and DYNAMIC/STATIC_GRIP values
## common value range N/A since it differs per car; mass and acceleration dependent
patch	float	bin:0x22658	0.45
patch	float	bin:0x2265c	1
patch	float	bin:0x22660	1.1
patch	float	bin:0x22664	1.35

## DYNAMIC_GRIP; amount of friction the tires produce when traction is broken, ie when the car is sliding or in a burnout
## common value range N/A since it differs per car; mass and acceleration dependent
patch	float	bin:0x22670	2
patch	float	bin:0x22674	2.05

## RIM_SIZE; self-explanatory; measured in inches
## common value range is 2x16-2x19
patch	float	bin:0x22680	18
patch	float	bin:0x22684	18

## YAW_SPEED; self-explanatory; rate at which car enters yaw state
## common value range is 0.30-0.70
patch	float	bin:0x2269c	0.325

## ASPECT_RATIO; self-explanatory; ratio of section height to section width
## common value range is 2x30-2x55
patch	float	bin:0x22678	40
patch	float	bin:0x2267c	40

## STATIC_GRIP; static grip is the amount of friction the tires are able to produce when they are not spinning, though they can be rolling
## common value range N/A since it differs per car; mass and acceleration dependent
patch	float	bin:0x22688	2.25
patch	float	bin:0x2268c	2.25

## GRIP_SCALE; tire grip scaling per axle
## common value range is 2x1.00-2x1.10
patch	float	bin:0x22668	1.185
patch	float	bin:0x2266c	1.2

## STEERING; steering ratio; value of 1.00 means that turning steering wheel by 360 degrees will turn wheels by 36 degrees
## common value range is 0.90-1.10
patch	float	bin:0x22698	1.05


##---------------------------------------------------
## Node: tires/default/punto/punto_top
##---------------------------------------------------

## SECTION_WIDTH
patch	float	bin:0x23040	245
patch	float	bin:0x23044	245

## YAW_CONTROL
patch	float	bin:0x23008	0.2
patch	float	bin:0x2300c	0.75
patch	float	bin:0x23010	0.85
patch	float	bin:0x23014	1

## DYNAMIC_GRIP
patch	float	bin:0x23020	2.2
patch	float	bin:0x23024	2.2

## RIM_SIZE
patch	float	bin:0x23030	18
patch	float	bin:0x23034	18

## YAW_SPEED
patch	float	bin:0x2304c	0.325

## ASPECT_RATIO
patch	float	bin:0x23028	40
patch	float	bin:0x2302c	40

## STATIC_GRIP
patch	float	bin:0x23038	2.3
patch	float	bin:0x2303c	2.4

## GRIP_SCALE
patch	float	bin:0x23018	1.2
patch	float	bin:0x2301c	1.2

## STEERING
patch	float	bin:0x23048	1.05


##---------------------------------------------------
## Node: transmission/default/punto
##---------------------------------------------------

## GEAR_COUNT; 1st GEAR_RATIO offset -6; total amount of gears including reverse, neutral and forward gears
## maximum number of elements is 11 but only 10 are proven to cause no problems with car drivability
## common value range is 7-9
patch	int16	bin:0x1eaca	8

## GEAR_RATIO; drivetrain power transfer ratios
## common value range N/A since it differs per car
patch	float	bin:0x1ead0	2.625
patch	float	bin:0x1ead4	0
patch	float	bin:0x1ead8	3.75
patch	float	bin:0x1eadc	2.36
patch	float	bin:0x1eae0	1.685
patch	float	bin:0x1eae4	1.312
patch	float	bin:0x1eae8	1.07
patch	float	bin:0x1eaec	0.85
patch	float	bin:0x1eaf0	0

## DIFFERENTIAL; self-explanatory; differential bias; 0.00 for rear, 0.50 for mid and 1.00 for front
## setting towards front will lock the front wheels more, causing the car to be prone to oversteer; inverse effect if bias set towards rear
## common value range is 2x0.60-2x0.80; 3x0.60-3x0.80 if car is AWD
patch	float	bin:0x1eafc	0.85
patch	float	bin:0x1eb00	0.85
patch	float	bin:0x1eb04	0.85

## GEAR_EFFICIENCY; overall power multiplier on current gear and rpm used to quickly change speed at each gear without any major reconfigurations
## common value set is 9x1.00
patch	float	bin:0x1eb10	1
patch	float	bin:0x1eb14	1
patch	float	bin:0x1eb18	1
patch	float	bin:0x1eb1c	1
patch	float	bin:0x1eb20	1
patch	float	bin:0x1eb24	1
patch	float	bin:0x1eb28	1
patch	float	bin:0x1eb2c	1
patch	float	bin:0x1eb30	1

## TORQUE_CONVERTER; percentage ratio of torque converter efficiency with automatic transmission usage
## common value range is 0.20-0.80
patch	float	bin:0x1eb34	0.45

## TORQUE_SPLIT; torque-to-axle transfer ratio; 0 for RWD, 0.5 for AWD and 1 for FWD
## common value range N/A since it differs per car
patch	float	bin:0x1eb38	0.5

## CLUTCH_SLIP; self-explanatory; manual gearbox efficiency ratio
## common value range is 0.70-0.90
patch	float	bin:0x1eb3c	0.85

## SHIFT_SPEED; shifting interval; stock [should be] higher than upgraded
## common value range is 0.10-0.25
patch	float	bin:0x1eb44	0.25

## FINAL_GEAR; final gear ratio determining top speed
## common value range N/A since it differs per car
patch	float	bin:0x1eb48	3.77


##---------------------------------------------------
## Node: transmission/default/punto/punto_top
##---------------------------------------------------

## GEAR_COUNT; 1st GEAR_RATIO offset -6
patch	int16	bin:0x20492	8

## GEAR_RATIO
patch	float	bin:0x20498	2.625
patch	float	bin:0x2049c	0
patch	float	bin:0x204a0	3.75
patch	float	bin:0x204a4	2.36
patch	float	bin:0x204a8	1.685
patch	float	bin:0x204ac	1.312
patch	float	bin:0x204b0	1.07
patch	float	bin:0x204b4	0.85
patch	float	bin:0x204b8	0

## DIFFERENTIAL
patch	float	bin:0x204c4	0.85
patch	float	bin:0x204c8	0.85
patch	float	bin:0x204cc	0.85

## GEAR_EFFICIENCY
patch	float	bin:0x204d8	1
patch	float	bin:0x204dc	1
patch	float	bin:0x204e0	1
patch	float	bin:0x204e4	1
patch	float	bin:0x204e8	1
patch	float	bin:0x204ec	1
patch	float	bin:0x204f0	1
patch	float	bin:0x204f4	1
patch	float	bin:0x204f8	1

## TORQUE_CONVERTER
patch	float	bin:0x204fc	0.45

## TORQUE_SPLIT
patch	float	bin:0x20500	0.5

## CLUTCH_SLIP
patch	float	bin:0x20504	0.8

## SHIFT_SPEED
patch	float	bin:0x2050c	0.25

## FINAL_GEAR
patch	float	bin:0x20510	3


##----------------------------------------------------
## Node: light_flares_cg/0xa95ab5ad; headlights setup
##----------------------------------------------------

## type
patch	float	bin:0x1842c	0

## 0xf7649e63; Size
patch	float	bin:0x18434	40

## Power
patch	float	bin:0x18428	0.1

## ZBias
patch	float	bin:0x18438	1.0


##----------------------------------------------------
## Node: light_flares_cg/brakelight_inner
##----------------------------------------------------

## Power
patch	float	bin:0x18728	0.1

## ZBias
patch	float	bin:0x18738	1.0


##----------------------------------------------------
## Node: light_flares_cg/reverselight_inner
##----------------------------------------------------

## Power
patch	float	bin:0x18728	0.1

## ZBias
patch	float	bin:0x18738	1.0


##----------------------------------------------------
## Node: emitterdata/default/emcar_nos_fire
##----------------------------------------------------

## Gravity
patch	float	bin:0x44758	0.5


##----------------------------------------------------
## Node: emitterdata/default/emcar_nos_glow
##----------------------------------------------------

## Gravity
patch	float	bin:0x442d8	0.5



MD5 hash: 4372656174656420627920464F58

