How to Install:
Step 1: Run Binary.

Step 2: In the binary interface move to "Binary Install" folder for the .end named "Install", select it and install. (It will flag an Error but you should ignore it).

Step 3: Depending on your vinyls. Go to the -512x or 1024x- folder and copy the car folder to the address where you installed the car.

Step 4: Run VLTED and select the NFSMS script and choose "install".

Step 5: Save the changes by pressing "Ctrl + S".

How to Delete:

-Simply repeat step two but this time choose "Binary Unistall",

-In VLTED select the option mentioned "Unistall" and save the changes by pressing "Ctrl + S".